Circulating pumps of CV type are provided for forced water circulation in the warmwater, heating and climatisation systems. Flow max. to 14 m3/h, pressure max. to 5.8 m WC. Allowable operation temperature up to 110°C.