Circulating pumps of GHN and GHNO type are provided for forced water circulation in the warmwater, heating, ventilation and climatisation systems. Flow max. to 6 m3/h, pressure max. to 6 m WC. Allowable operation temperature up to 110°C.