Circulating pumps of CB, CBK and CBP type are provided for forced water circulation in the warmwater, heating, ventilation and climatisation systems. Models CBK and CBP are also suitable for non-aggressive fluids in industry. Flow max. to 180 m3/h, pressure max. to 56 m WC. Allowable operation temperature up to 140°C.