Circulating pumps of GHN and GHNO type are provided for forced water circulation in the industry for non-aggressive fluids. Flow max. to 180 m3/h, pressure max. to 56 m WC. Allowable operation temperature up to 140°C.