Circulating pumps of CL type are provided for forced water circulation in the warmwater, heating, ventilation and climatisation systems. Flow max. to 200 m3/h, pressure max. to 60 m WC. Allowable operation temperature up to 140°C.